PCB-1.99j-mag1 command reference ©1998, 1999, 2000, 2001 harry eaton

misc operations backspace remove object [S][C]Btn1 remove object scroll wheel vertical pan [S]scroll wheel horizontal pan Btn1 current mode action u undo operation [S]r redo operation [S][C]u clear undo-list tab switch viewing side cursor key move crosshair 1 grid [S]cursor key move crosshair 10 grid

connections [S]f reset found connections f find connections [S]backspace remove connections

user (:) commands :DRC() check layout for rule violations :l [file] load data file :le [file] load element to buffer :m [file] load layout to buffer :q quit application :rn [file] load netlist :s [file] save data as file

display c center display g increase grid spacing [S]g decrease grid spacing [C]m mark location r clear and redraw output z zoom in [S]z zoom out v zoom extents [S]Btn3 temporary zoom extents selection Btn2 select/deselect object [S]Btn2 toggle object to selection drag Btn2 select only objects in box drag [S]Btn2 add box to selection [S]m move selected to current layer

copy and move drag Btn2 move object or selection drag [M]Btn2 copy object drag [S][M]Btn2 override rubberband & move m move to current layer

pastebuffer [C]x copy selected objects to buffer and enter pastebuffer mode [S][C]x cut selected objects to buffer and enter pastebuffer mode Btn1 in pastebuffer mode copy to layout [C]1· · ·5 select buffer # 1· · ·5

sizing s increase size of TLAPV^a [S]s decrease size of TLAPV [M]s increase drill size of PV [S][M]s decrease drill size of PV k increase clearance of LAPV [S] k decrease clearance of LAPV

element d display pinout [S]d open pinout window h hide/show element name n change element name

pin/pad n change name q toggle square flag

aTLAPV: text, line, arc, pin or via via F1 enter via-mode [C]v increase initial size [S][C]v decrease initial size [M]v inc. initial drilling hole [S][M]v dec. initial drilling hole [C]h convert via to mounting hole

lines/arcs F2 enter line mode F3 enter arc mode l increase initial line size [S]l decrease initial line size period toggle 45 degree enforcement / cycle multiline mode [S] override multiline mode

polygon F5 enter rectangle-mode F6 enter polygon-mode [S]p close path insert enter insert point mode

text F4 enter text-mode n edit string t increase initial text size [S]t decrease initial text size

rats nest w add all rats [S]w add rats to selected pins/pads e delete all rats [S]e delete selected rats o optimize all rats [S]o optimize selected rats

Obviously [S], [C], [M], F and Btn mean the shift, control, modifier1 (BTNMOD for buttons), function key and mouse button.

2